|  | Home · All Classes · Main Classes · Grouped Classes · Modules · Functions |

[Contents]

# Environment Variables

Variable | Description
--- | ---
QWS_SW_CURSOR | If defined, always use a software mouse cursor even when using an accelerated driver that supports a hardware cursor.
QWS_DISPLAY | Specifies the display type and framebuffer. For example, if the current shell is bash, ksh, zsh or sh:
        export QWS_DISPLAY=<gfx driver><:driver specific options><:display number>
The default value is an unaccelerated Linux framebuffer driver: `/dev/fb0`. Valid drivers are `QVfb`, `LinuxFb` (unaccelerated Linux framebuffer), `Transformed` (for rotated displays), and `VNC` (when running Qtopia Core as a VNC server). Transformed displays have a special format: the specification should include a rotation as a multiple of 90 degrees given as `rot<x>`, for instance `transformed:rot90`. See also Running Applications, The Virtual Framebuffer and The VNC Protocol.
QWS_SIZE | Specifies the size of Qtopia Core's window which is centered within the screen. For example, if the current shell is bash, ksh, zsh or sh:
        export QWS_SIZE=<width>x<height>
QWS_MOUSE_PROTO | Specifies the driver and device for pointer handling. For example, if the current shell is bash, ksh, zsh or sh:
        export QWS_MOUSE_PROTO=<driver>:<device>
The available drivers are `MouseMan`, `IntelliMouse`, `Microsoft`, `VR41xx`, `LinuxTP` or `Tslib`, and the device is typically `/dev/mouse`, or `/dev/ts` for touch panels. Note that specifying the device is optional. The default value is `Auto` which enables auto-detection of the mouse device if the "pc" mouse driver is enabled. Note that Qtopia Core does not support auto-detection of touch panels in which case the driver must be specified explicitly to determine which device to use. See also Pointer Handling.
QWS_KEYBOARD | Specifies the driver and device for character input. For example, if the current shell is bash, ksh, zsh or sh:
        export QWS_KEYBOARD=<driver>:<device>
The available drivers are `SL5000`, `Yopy`, `VR41xx`, `TTY` or `USB`, and the device is typically `/dev/tty0`. Note that specifying the device is optional. Multiple keyboard drivers can be specified in one go:
        export QWS_KEYBOARD=<driver> <driver> <driver>:<device>
Input will be read from all of specified drivers. See also Character Input.

[Contents]