/****************************************************************************
**
** This file is part of Qt Creator
**
** Copyright (c) 2011 Nokia Corporation and/or its subsidiary(-ies).
**
** Contact: Nokia Corporation (qt-info@nokia.com)
**
**
** GNU Free Documentation License
**
** Alternatively, this file may be used under the terms of the GNU Free
** Documentation License version 1.3 as published by the Free Software
** Foundation and appearing in the file included in the packaging of this
** file.
**
** If you have questions regarding the use of this file, please contact
** Nokia at qt-info@nokia.com.
**
****************************************************************************/

    /*!

    \contentspage index.html
    \previouspage creator-developing-meego.html
    \page creator-developing-generic-linux.html
    \nextpage creator-developing-maemo.html

    \title Connecting Generic Linux Devices

    You can connect generic Linux devices to the development PC to build, run,
    debug, and analyze applications on them from \QC.

    If you have the tool chain for building applications for generic Linux
    devices (with no MADDE support) installed on the development PC, you can add
    it to \QC.

    To be able to run and debug applications on generic Linux devices, you must
    create device configurations and select them in the \QC run
    settings.

    You use a wizard to create the connections. You can edit the settings later
    in \gui {Tools > Options > Linux Devices > Device Configurations}.

    \image qtcreator-linux-device-configurations.png "Device Configurations dialog"

    You can protect the connections between \QC and a device by using
    either a password or an SSH key. If you do not have an SSH key, you can
    create it in \QC. For more information, see \l {Generating SSH Keys}.

    To configure connections between \QC and generic Linux devices:

    \list 1

        \o  Make sure that your device can be reached via an IP address.

        \o  Select \gui {Tools > Options > Build & Run > Qt Versions > Add} to
            add the Qt version
            for the generic Linux.

        \o  Select \gui {Tools > Options > Build & Run > Tool Chains > Add} to
            add the tool
            chain for building the applications.

        \o  To deploy applications and run them remotely on devices, specify
            parameters for accessing the devices:

            \list 1

                \o  Select \gui {Tools > Options > Linux Devices > Device
                    Configurations > Add > Generic Linux Device > Start Wizard}.

                    \image qtcreator-screenshot-devconf-linux.png "Connection Data wizard"

                \o  In the \gui {The name to identify this configuration} field,
                    enter a name for the connection.

                \o  In the \gui {The device's host name or IP address} field,
                    enter the host name or IP address of the device.

                \o  In the \gui {The user name to log into the device} field,
                    enter the user name to log into the device and run the
                    application as.

                \o  In the \gui {The authentication type} field, select whether
                    to use \gui Password or \gui Key authentication, and enter
                    the user's password or the file that contains the user's
                    private key.

                \o Click \gui {Next} to create the connection.

            \endlist

        \o  To specify build settings:

        \list 1

            \o  Open a project for an application you want to develop for the
                device.

            \o  Select \gui {Projects > Desktop > Build}.

            \o  Select the Qt version and tool chain for the generic Linux
                device.

        \endlist

        \o To specify run settings:

        \list 1

            \o  Select \gui {Run > Add > Build Tarball and Deploy to Linux Host}
                to add a new deploy configuration.

                \image qtcreator-run-settings-linux-devices.png "Run settings for generic Linux devices"

            \o  In the \gui {Device configuration} field, select the device
                connection.

        \endlist

        When you run the project, \QC creates an installation package in
        the build directory. The name of the directory is displayed in the
        \gui {Create tarball} step.

        The \gui {Deploy tarball via SFTP upload using device} step specifies
        that \QC uploads the tarball to the device and extracts it.
                You can add custom deploy steps and remove the default step if
                it is incompatible with your steps.
                To only create a tarball and not copy the files to the device,
                remove all deploy steps.

    \endlist

*/

