/****************************************************************************
**
** Copyright (C) 2013 Aaron McCarthy <mccarthy.aaron@gmail.com>
** Copyright (C) 2017 The Qt Company Ltd.
** Contact: https://www.qt.io/licensing/
**
** This file is part of the documentation of the Qt Toolkit.
**
** $QT_BEGIN_LICENSE:FDL$
** Commercial License Usage
** Licensees holding valid commercial Qt licenses may use this file in
** accordance with the commercial license agreement provided with the
** Software or, alternatively, in accordance with the terms contained in
** a written agreement between you and The Qt Company. For licensing terms
** and conditions see https://www.qt.io/terms-conditions. For further
** information use the contact form at https://www.qt.io/contact-us.
**
** GNU Free Documentation License Usage
** Alternatively, this file may be used under the terms of the GNU Free
** Documentation License version 1.3 as published by the Free Software
** Foundation and appearing in the file included in the packaging of
** this file. Please review the following information to ensure
** the GNU Free Documentation License version 1.3 requirements
** will be met: https://www.gnu.org/licenses/fdl-1.3.html.
** $QT_END_LICENSE$
**
****************************************************************************/

/*!
\page qtnfc-index.html
\title Qt NFC
\brief Enables connectivity between NFC enabled devices.
\ingroup technology-apis

The NFC API provides connectivity between NFC enabled devices.

Currently the API is supported on \l{Qt for Android}{Android},
and \l{Qt for Linux/X11}{Linux} using \l {https://01.org/linux-nfc}{Neard} v0.14 or later.

\section1 Overview

NFC is an extremely short-range (less than 20 centimeters) wireless technology and has a
maximum transfer rate of 424 kbit/s. NFC is ideal for transferring small packets of data when two
devices are touched together.

The NFC API provides APIs for interacting with NFC Forum Tags and NFC Forum Devices, including
target detection and loss, registering NDEF message handlers, reading and writing NDEF messages
on NFC Forum Tags and sending tag specific commands.


\section1 Getting Started

To use the C++ library in your application, add the following configuration
option to your \c .pro file:

\snippet snippets.pro project modification

To use the classes of the module in your application you need the following
import statement in your \c .qml file:

\snippet doc_src_qtnfc.qml import

\section1 Related Information

\section2 Guides
\list
    \li \l {Qt NFC Overview}
\endlist

\section2 Reference
\list
    \li \l {Qt NFC QML Types}{QML Types}
    \li \l {Qt NFC C++ Classes}{C++ Classes}
\endlist

\section2 Logging Categories

The \l QtNfc module exports the following
\l {Configuring Categories}{logging categories}:

\table
\header
    \li Logging Category
    \li Description
\row
    \li qt.nfc.neard
    \li Enables logging of the Neard/Linux implementation
\endtable

\section2 Examples
\list
    \li QML
    \list
        \li \l {corkboard}{CorkBoard}
        \li \l {poster}{QML Poster}
    \endlist
    \li C++
    \list
        \li \l {annotatedurl}{Annotated URL}
        \li \l {ndefeditor}{NDEF Editor}
    \endlist
\endlist
*/
