# TIFFBUFFER

NAME
SYNOPSIS
DESCRIPTION
DIAGNOSTICS
SEE ALSO

## NAME

| TIFFReadBufferSetup, TIFFWriteBufferSetup − I/O buffering control routines

## SYNOPSIS

    #include <tiffio.h>

    int TIFFReadBufferSetup(TIFF *tif, tdata_t buffer, tsize_t size);
    int TIFFWriteBufferSetup(TIFF *tif, tdata_t buffer, tsize_t size);

## DESCRIPTION

| The following routines are provided for client-control of the I/O buffers used by the library. Applications need never use these routines; they are provided only for ‘‘intelligent clients’’ that wish to optimize memory usage and/or eliminate potential copy operations that can occur when working with images that have data stored without compression. TIFFReadBufferSetup sets up the data buffer used to read raw (encoded) data from a file. If the specified pointer is NULL (zero), then a buffer of the appropriate size is allocated. Otherwise the caller must guarantee that the buffer is large enough to hold any individual strip of raw data. TIFFReadBufferSetup returns a non-zero value if the setup was successful and zero otherwise. TIFFWriteBufferSetup sets up the data buffer used to write raw (encoded) data to a file. If the specified size is −1 then the buffer size is selected to hold a complete tile or strip, or at least 8 kilobytes, whichever is greater. If the specified buffer is NULL (zero), then a buffer of the appropriate size is dynamically allocated. TIFFWriteBufferSetup returns a non-zero value if the setup was successful and zero otherwise.

## DIAGNOSTICS

| %s: No space for data buffer at scanline %ld. TIFFReadBufferSetup was unable to dynamically allocate space for a data buffer. %s: No space for output buffer. TIFFWriteBufferSetup was unable to dynamically allocate space for a data buffer.

## SEE ALSO

| libtiff(3TIFF) Libtiff library home page: http://www.remotesensing.org/libtiff/